Cmp-Mod V01 Created by PcbNew   date = 2018 December 08, Saturday 11:39:52

BeginCmp
TimeStamp = 5C247A81
Path = 
Reference = REF**;
ValeurCmp = RESET;
IdModule  = Button_Switch_THT:Reset;
EndCmp

BeginCmp
TimeStamp = 5C081AB8
Path = 
Reference = ProMicro;
ValeurCmp = [NoVal];
IdModule  = promicro:ProMicro;
EndCmp

BeginCmp
TimeStamp = 5BF02D03
Path = 
Reference = D8;
ValeurCmp = [NoVal];
IdModule  = Diode_THT:D_5W_P10.16mm_Horizontal;
EndCmp

BeginCmp
TimeStamp = 5BF02CE5
Path = 
Reference = D7;
ValeurCmp = [NoVal];
IdModule  = Diode_THT:D_5W_P10.16mm_Horizontal;
EndCmp

BeginCmp
TimeStamp = 5BF02CCE
Path = 
Reference = SW8;
ValeurCmp = [NoVal];
IdModule  = Button_Switch_Keyboard:SW_Cherry_MX1A_1.00u_Plate;
EndCmp

BeginCmp
TimeStamp = 5BF02CB7
Path = 
Reference = SW7;
ValeurCmp = [NoVal];
IdModule  = Button_Switch_Keyboard:SW_Cherry_MX1A_1.00u_Plate;
EndCmp

BeginCmp
TimeStamp = 5BF02C99
Path = 
Reference = D9;
ValeurCmp = [NoVal];
IdModule  = Diode_THT:D_5W_P10.16mm_Horizontal;
EndCmp

BeginCmp
TimeStamp = 5BF02C82
Path = 
Reference = SW9;
ValeurCmp = [NoVal];
IdModule  = Button_Switch_Keyboard:SW_Cherry_MX1A_1.00u_Plate;
EndCmp

BeginCmp
TimeStamp = 5BF02D03
Path = 
Reference = D5;
ValeurCmp = [NoVal];
IdModule  = Diode_THT:D_5W_P10.16mm_Horizontal;
EndCmp

BeginCmp
TimeStamp = 5BF02CE5
Path = 
Reference = D4;
ValeurCmp = [NoVal];
IdModule  = Diode_THT:D_5W_P10.16mm_Horizontal;
EndCmp

BeginCmp
TimeStamp = 5BF02CCE
Path = 
Reference = SW5;
ValeurCmp = [NoVal];
IdModule  = Button_Switch_Keyboard:SW_Cherry_MX1A_1.00u_Plate;
EndCmp

BeginCmp
TimeStamp = 5BF02CB7
Path = 
Reference = SW4;
ValeurCmp = [NoVal];
IdModule  = Button_Switch_Keyboard:SW_Cherry_MX1A_1.00u_Plate;
EndCmp

BeginCmp
TimeStamp = 5BF02C99
Path = 
Reference = D3;
ValeurCmp = [NoVal];
IdModule  = Diode_THT:D_5W_P10.16mm_Horizontal;
EndCmp

BeginCmp
TimeStamp = 5BF02C82
Path = 
Reference = SW6;
ValeurCmp = [NoVal];
IdModule  = Button_Switch_Keyboard:SW_Cherry_MX1A_1.00u_Plate;
EndCmp

BeginCmp
TimeStamp = 5BF029FF
Path = 
Reference = D3;
ValeurCmp = [NoVal];
IdModule  = Diode_THT:D_5W_P10.16mm_Horizontal;
EndCmp

BeginCmp
TimeStamp = 5BF029E8
Path = 
Reference = SW3;
ValeurCmp = [NoVal];
IdModule  = Button_Switch_Keyboard:SW_Cherry_MX1A_1.00u_Plate;
EndCmp

BeginCmp
TimeStamp = 5BF029FF
Path = 
Reference = D2;
ValeurCmp = [NoVal];
IdModule  = Diode_THT:D_5W_P10.16mm_Horizontal;
EndCmp

BeginCmp
TimeStamp = 5BF029E8
Path = 
Reference = SW2;
ValeurCmp = [NoVal];
IdModule  = Button_Switch_Keyboard:SW_Cherry_MX1A_1.00u_Plate;
EndCmp

BeginCmp
TimeStamp = 5BF02667
Path = 
Reference = SW1;
ValeurCmp = [NoVal];
IdModule  = Button_Switch_Keyboard:SW_Cherry_MX1A_1.00u_Plate;
EndCmp

BeginCmp
TimeStamp = 5BF028A1
Path = 
Reference = D1;
ValeurCmp = [NoVal];
IdModule  = Diode_THT:D_5W_P10.16mm_Horizontal;
EndCmp

BeginCmp
TimeStamp = 5BFC8152
Path = 
Reference = [NoRef];
ValeurCmp = [NoVal];
IdModule  = MountingHole:MountingHole_3.2mm_M3;
EndCmp

BeginCmp
TimeStamp = 5BFC81A4
Path = 
Reference = [NoRef];
ValeurCmp = [NoVal];
IdModule  = MountingHole:MountingHole_3.2mm_M3;
EndCmp

BeginCmp
TimeStamp = 5BFC8248
Path = 
Reference = [NoRef];
ValeurCmp = [NoVal];
IdModule  = MountingHole:MountingHole_3.2mm_M3;
EndCmp

BeginCmp
TimeStamp = 5BFC8257
Path = 
Reference = [NoRef];
ValeurCmp = [NoVal];
IdModule  = MountingHole:MountingHole_3.2mm_M3;
EndCmp

EndListe
